Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Remove a RIP Neighbor

In this example, switch 2 is removed from switch 1.

1. On switch 1, enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1

2. Delete the configured RIP neighbor.

       SEFOS(config-router)# no neighbor 10.0.0.2
       SEFOS(config-router)# end

   In switch 1, you should be able to view the routes that are sent as RIP updates from both of the neighbor routers (switch 2 at `10.0.0.2` and switch 3 at `10.0.0.3`).

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |