Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### Component Sensor Targets

Use the targets from this table to check the switch status. See Check Switch Status (Oracle ILOM).

Component Sensor | Target | Comment
--- | --- | ---
Chassis fault | `/SYS/SERVICE` |
Chassis locator | `/SYS/LOCATE` |
Chassis OK | `/SYS/OK` |
Fan fault | `/SYS/FM` x`/SERVICE` | where x is 0-4
Fan presence | `/SYS/FM` x`/PRSNT` | where x is 0-4
Fan speed | `/SYS/FM` x`/TACH` | where x is 0-4
Power supply fault | `/SYS/PS` y`/SERVICE` | where y is 0 or 1
Power supply presence | `/SYS/PS` y`/PRSNT` | where y is 0 or 1
Power supply speed | `/SYS/PS` y`/OK` | where y is 0 or 1

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |