Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable DCB for Each Interface

This example uses port 0/2.

1. Enter Global Configuration mode.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/2

2. Disable DCB.

       SEFOS(config-if)# set dcb disable

3. Exit Global Configuration mode.

       SEFOS(config-if)# end

4. View the interface DCB state after it was disabled.

       SEFOS# show interfaces extreme-ethernet 0/2 dcb mode

       Port                  : Ex0/2
       Show Type             : Admin State
       DCB Capable State     : off
       Priority Group        : auto
       Priority Flow Control : auto

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |