Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

##### Rear Panel LEDs

The power supply status LEDs and fan status LEDs are located on the rear of the switch.

No. | Name | Color | State and Meaning
--- | --- | --- | ---
1 | Power Supply OK | Green | On – Power supply is functional without fault. Off – Power supply is off or initializing.
2 | Power Supply Attention | Yellow | On – Fault detected, 12 VDC shut down. Off – No faults detected.
3 | Power Supply AC | Green | On – AC is functional without fault. Off – AC is off or initializing.
4 | Fan Fault | Yellow | On – Fan has a fault. Off – No fault detected.

##### Related Information

- Front Panel LEDs

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |