Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure SEFOS1

Use the following commands to configure `VLAN 50` and `VLAN 40` on switch SEFOS1 in the example topology.

1. Configure SEFOS1.

       SEFOS 1 SEFOS# configure terminal
       SEFOS 1 SEFOS(config)# set gvrp disable
       SEFOS 1 SEFOS(config)# set gmrp disable

       SEFOS 1 SEFOS(config)# interface extreme-ethernet 0/15
       SEFOS 1 SEFOS(config-if)# switchport access vlan 50
       % Access VLAN does not exist.,Creating vlan
       SEFOS 1 SEFOS(config-if)# exit

       SEFOS 1 SEFOS(config)# interface vlan 50
       SEFOS 1 SEFOS(config-if)# no shutdowndown
       SEFOS 1 SEFOS(config-if)# ipv6 enable
       SEFOS 1 SEFOS(config-if)# ipv6 address  5555::14 112
       SEFOS 1 SEFOS(config-if)# exit

       SEFOS 1 SEFOS(config)# vlan 40
       SEFOS 1 SEFOS(config-vlan)# port extreme-ethernet 0/3
       SEFOS 1 SEFOS(config-vlan)# exit

       SEFOS 1 SEFOS(config)# interface extreme-ethernet 0/3
       SEFOS 1 SEFOS(config-if)# no shut
       SEFOS 1 SEFOS(config-if)# exit

       SEFOS 1 SEFOS(config)# interface vlan 40
       SEFOS 1 SEFOS(config-if)# no shut
       SEFOS 1 SEFOS(config-if)# ipv6 enable
       SEFOS 1 SEFOS(config-if)# ipv6 address 4444::14 112
       SEFOS 1 SEFOS(config-if)# end

       SEFOS 1 SEFOS# configure terminal
       SEFOS 1 SEFOS(config)# vlan 30
       SEFOS 1 SEFOS(config-vlan)# port extreme-ethernet 0/7
       SEFOS 1 SEFOS(config-vlan)# exit

       SEFOS 1 SEFOS(config)# interface extreme-ethernet 0/7
       SEFOS 1 SEFOS(config-if)# no shut
       SEFOS 1 SEFOS(config-if)# exit

       SEFOS 1 SEFOS(config)# interface vlan 30
       SEFOS 1 SEFOS(config-if)# no shut
       SEFOS 1 SEFOS(config-if)# ipv6 enable
       SEFOS 1 SEFOS(config-if)# ipv6 address 3333::14 112
       SEFOS 1 SEFOS(config-if)# end
       SEFOS 1 SEFOS#

2. Show the status of IPv6 interfaces on SEFOS1.

       SEFOS 1 SEFOS# show ipv6 interface
       vlan1 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::221:28ff:fe56:d7a9
           Global unicast address(es):
               Not Configured.
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::1:ff56:d7a9
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan50 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::221:28ff:fe56:d7a9
           Global unicast address(es):
               5555::14/112
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::1:ff00:14
               ff02::1:ff56:d7a9
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan40 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::221:28ff:fe56:d7a9
           Global unicast address(es):
               4444::14/112
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::1:ff00:14
               ff02::1:ff56:d7a9
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan30 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::221:28ff:fe56:d7a9
           Global unicast address(es):
               3333::14/112
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::1:ff00:14
               ff02::1:ff56:d7a9
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |