Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

## Create Multiple LBGs

To create more than one LBG, you can execute the `slb` command as shown in previous sections, with a different VIP or VIP address mask. This example forms two LBGs, each with two server members.

- Type.

      SEFOS# configure terminal
      SEFOS(config)# slb 10.10.10.0 255.255.255.0 192.0.0.1,192.0.0.2
      SEFOS(config)# slb 10.10.11.0 255.255.255.0 192.0.0.3,192.0.0.4
      SEFOS(config)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |