Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Redistribution Configuration

This procedure configures the information to be applied to routes learned from the RTM.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

3. Configure the ASBR router.

       SEFOS(config-router)# asbr outer

4. Configure the redistribution of static routes.

       SEFOS(config-router)# redistribute static

5. Configure the redistribution configuration.

       SEFOS(config-router)# redist-config 20.0.0.0 255.0.0.0 metric-value     100 metric-type asExttype1 tag 10

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |