Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Power Off a Power Supply

Note - Powering off both power supplies powers off the switch.

1. Determine which power supply is to be removed.
2. At the rear of the switch chassis, remove the power cord from the respective power supply.

   The power supply is completely powered off.

3. Remove the power supply.

   See Remove a Power Supply.

##### Related Information

- Remove a Power Supply

- Install a Power Supply

- Power On a Power Supply

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |