Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Log Into Oracle ILOM Web (NET MGT)

1. Obtain the IP address or host name of your SP.

   See:

   - Verify the DHCP-Assigned IP Address and Host Name

   - Configure Network Management From CLI (SER MGT)

2. Configure an externally accessible IP address on the switch.

   Perform the appropriate task described in Connecting to the Service Processor.

3. Type the IP address of the switch into your web browser.

   The login screen appears.

4. Type your user name and password.

   When you first try to access the web interface, it prompts you to type the default user name and password. The default user name and password are:

   - Default user name: `root`

   - Default password: `changeme`

     The default user name and password are in lowercase characters.

5. Click Log In.

   The web interface appears.

6. Access SEFOS.

##### Related Information

- Oracle ILOM Overview

- Verify the DHCP-Assigned IP Address and Host Name

- Configure Network Management From CLI (SER MGT)

- Log Into Oracle ILOM CLI (NET MGT)

- Log Into Oracle ILOM CLI (SER MGT)

- Configure Network Management From Web

- Configure Network Management From CLI (NET MGT)

- Log Out of ILOM

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |