Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System Uplink Port Trailing Administration Guide

Search Scope:

- This Document
- Entire Library

### Verify the Configurations

1. Check the Uplink Port Trailing feature status.

       NEM24p-0 SEFOS# show uplink-trailing global
       % Uplink Trailing enabled

2. Verify the configuration of all groups configured on this switch.

       NEM24p-0 SEFOS# show uplink-trailing group summary
       Uplink Trailing Group 10
       Description:     Uplink-trailing between NEM24p-0 & ToR72p-1
               Admin Status:            Enabled
               Status:                  Up

       Port             Type   Status
       Ex0/1        uplink      Up
       Ex0/18       downlink    Up

       NEM24p-0 SEFOS# show uplink-trailing group detail
       Uplink Trailing Group 10
       Description:     Uplink-trailing between NEM24p-0 & ToR72p-1
               Admin Status:            Enabled
               Status:                  Up
       Link State Change: Up   1       Down    0

       Port             Type   Status
       Ex0/1        uplink      Up
       Ex0/18       downlink    Up

3. Verify the configuration of a particular group.

       NEM24p-0 SEFOS# show uplink-trailing group 10
       Uplink Trailing Group 10
       Description:     Uplink-trailing between NEM24p-0 & ToR72p-1
               Admin Status:            Enabled
               Status:                  Up

       Port             Type   Status
       Ex0/1        uplink      Up
       Ex0/18       downlink    Up

       NEM24p-1 SEFOS# show uplink-trailing group 20
       Uplink Trailing Group 20
       Description:     Uplink-trailing between NEM24p-1 & ToR72p-1
               Admin Status:            Enabled
               Status:                  Up

       Port             Type   Status
       Ex0/1        uplink      Up
       Ex0/18       downlink    Up

4. Verify the Uplink Port trailing configuration on an interface.

       NEM24p-0 SEFOS# show uplink-trailing interface extreme-ethernet 0/1 summary
       Interface Ex0/1
       Uplink Trailing Group    10
       Port Type                uplink
       Port Link Status         Up

       NEM24p-0 SEFOS# show uplink-trailing interface extreme-ethernet 0/1 detail
       Interface Ex0/1
       Uplink Trailing Group    10
       Group Description:       Uplink-trailing between NEM24p-0 & ToR72p-1
       Group Admin Status:      Enabled
       Group Link Status:       Up
       Port Type                uplink
       Port Link Status         Up

       NEM24p-0 SEFOS#
       NEM24p-0 SEFOS# show uplink-trailing interface extreme-ethernet 0/18 detail
       Interface Ex0/18
       Uplink Trailing Group    10
       Group Description:       Uplink-trailing between NEM24p-0 & ToR72p-1
       Group Admin Status:      Enabled
       Group Link Status:       Up
       Port Type                downlink
       Port Link Status         Up

Copyright © 2015, Oracle and/or its affiliates. All rights reserved. Legal Notices |