Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable an Address Range

This example disables the entire range that is not to be advertised.

1. Disable a previously specified range so that it is not advertised.

       SEFOS(config-router)# area 0.0.0.0 summary-prefix 3333::  64 not-advertise

2. Verify that the database entry has been removed.

       SEFOS# show ipv6 ospf database as-external detail

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |