Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable IGMP Globally

You must enable IGMP globally and on the interface on which IGMP is needed. By default, IGMP is disabled globally.

1. Enable IGMP in the router.

       SEFOS# configure terminal
       SEFOS(config)# set ip igmp enable
       SEFOS(config)# end

2. Review the configuration information.

       SEFOS# show ip igmp global-config

       IGMP is globally enabled

   Note - To disable IGMP in the switch, execute the `set ip igmp disable` command.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |