Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RMON Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable the Ethernet Statistics Group

You can configure the collection of statistics over any port.

1. Enter Global Configuration mode.

       SEFOS# configure terminal

2. Enter Interface Configuration mode.

       SEFOS(config)# interface extreme-ethernet 0/15

3. Enable the statistics group on the specified interface (port 15).

       SEFOS(config-if)# rmon collection stats 1 owner myTest
       SEFOS(config-if)# exit
       SEFOS(config)# exit

4. Verify the entries.

       SEFOS# show rmon statistics 1

       RMON is enabled
       Collection 1 on EX0/15 is active, and owned by myTest,
       Monitors ifEntry.1.15 which has
        Received 1556 octets, 16 packets,
        1 broadcast and 0 multicast packets,
        0 undersized and 0 oversized packets,
        0 fragments and 0 jabbers,
        0 CRC alignment errors and 0 collisions.
        # of packets received of length (in octets):
        64: 2, 65-127: 14, 128-255: 0,
        256-511: 0, 512-1023: 0, 1024-1518: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |