Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

## Create SLB Server Members

When you add a server member as the first member of the group, an LBG is created. This example shows adding two server entries, as well as a single standby server, to an LBG.

1. Add the first and second server members.

       SEFOS# configure terminal
       SEFOS(config)# slb 10.10.10.0 255.255.255.0 192.0.0.1,192.0.0.2

2. Create a standby SLB server member.

       SEFOS# configure terminal
       SEFOS(config)# slb standby 10.10.10.0 255.255.255.0 192.0.0.3
       SEFOS(config)# end

3. Show current LBGs and members.

   The following example shows LBG with one active SLB server member and one standby SLB server member. For information about the status of a server member, see Conditions for a Member Participating in Load Distribution.

       SEFOS# show slb

       SLB Group ID: 1 Virtual IP: 10.10.10.0/24
       Server Members:
       IP Address       Vlan  MacAddress        Port State     Comments
       ================ ====  ================= ==== ========= ==================
       192.0.0.1            1  00:14:4f:3e:e0:10    3 ACTIVE
       192.0.0.2            1  00:14:4f:3e:e0:15    8 IDLE
       192.0.0.3            1  00:14:4f:3e:e0:19   12 STANDBY   (up)

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |