Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring RP-Candidate Behavior

You can configure an RP candidate to send periodic candidate-RP-advertisement messages to the BSR and to process JP or register messages for the advertised group prefix, when it is elected as an RP.

Use `RP-candidate RP-address` to configure the address of the interface that is advertised as a candidate-RP. In addition, you can specify the group address for which the entry that contains routing information and the group mask, which provides the group prefix for the entry that contains information about the RP.

- Specify the Address for the Candidate RP

- Delete an RP Candidate

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |