Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure SEFOS2

1. Configure the area.

       SEFOS# configure terminal
       SEFOS(config)# router ospf
       SEFOS(config-router)# router-id 10.4.0.2
       SEFOS(config-router)# network 10.4.0.2 area 0.0.0.0
       SEFOS(config-router)# network 10.2.2.2 area 0.0.0.2

2. Configure area `0.0.0.2` as an NSSA area.

       SEFOS(config-router)# area 0.0.0.2 nssa
       SEFOS(config-router)# exit

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |