Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LLDP System Control Status

This section describes how to configure the LLDP system control status, which is set to Start by default. You must set the LLDP system control status to Start before you make any configuration changes in LLDP.

1. In switch 1, shut down LLDP.

       SEFOS# configure terminal
       SEFOS(config)# shutdown lldp
       SEFOS(config)# end

2. View the LLDP system control status.

       SEFOS# show lldp

       % Lldp Module is shutdown

3. Start LLDP.

       SEFOS# configure terminal
       SEFOS(config)# no shutdown lldp
       SEFOS(config)# end

   After the LLDP system control status is changed to Start, LLDP global configuration objects are set with default values.

4. View the default values for the global configuration objects of LLDP.

       SEFOS# show lldp
       LLDP is disabled
       Transmit Interval        : 30
       Holdtime Multiplier        : 4
       Reinitialization Delay    : 2
       Tx Delay            : 2
       Notification Interval    : 5
       Chassis Id SubType        : Mac Address
       Chassis Id            : 00:01:02:03:04:01

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |