Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable Fast-Leave Processing

The fast-leave processing feature is disabled by default.

1. Enable fast-leave processing.

       SEFOS# configure terminal
       SEFOS(config)# vlan 4
       SEFOS(config-vlan)# ipv6 mld snooping fast-leave
       SEFOS(config-vlan)# end

2. View the configuration.

       SEFOS# show ipv6 mld snooping

       Snooping VLAN Configuration for the VLAN 4
         MLD Snooping enabled
         MLD Operating version is V2
         Fast leave is enabled
         Snooping switch is acting as Non-Querier
         Query interval is 125 seconds

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |