Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable a Multicast Router Port

1. Enter the configure mode for the VLAN.

       SEFOS# configure terminal
       SEFOS(config)# vlan 4

2. Disable the router port.

       SEFOS(config-vlan)# no ip igmp snooping mrouter extreme-ethernet 0/8
       SEFOS(config)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |