Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Display the Pseudo Root ID

This example displays the configured pseudo root ID if the port is configured as a L2GP only.

- Display the pseudo BPDU.

      SEFOS# show spanning-tree layer2-gateway-port

      Switch default
      Port Ex0/1
            PseudoRootId
      Priority       MacAddress
      ---------        ------------------
       4096         00:01:02:03:04:01

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |