Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Power On a Power Supply

1. Remove a power supply and install a new one.

   See:

   - Remove a Power Supply

   - Install a Power Supply

2. Reconnect the power cord to the power supply.

   The AC LED lights green to indicate the power supply is connected to facility power. A moment later, the OK LED lights green to indicate the power supply is at full power.

3. Verify the power supply’s operation.

##### Related Information

- Power Off a Power Supply

- Remove a Power Supply

- Install a Power Supply

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |