Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Delete a Static Route

This example deletes the static route for the SEFOS2 `VLAN 2` interface in the SEFOS1 routing table.

1. Delete the static route.

       SEFOS# configure terminal
       SEFOS(config)# no ipv6 route 3333:: 64 fec0::2856:0:2

2. Ensure that the static route was removed from the SEFOS1 routing table.

       SEFOS# show ipv6 route

       IPv6 Routing Table  -  2 entries
       Codes : C - Connected, S - Static
       C   fec0::1111:0:0/96   [1/1]
               via ::, vlan11
       C   fec0::2856:0:0/96   [1/1]
               via ::, vlan10

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |