Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Clear Snooping Statistics for a Specific VLAN

This example clears statistics for `VLAN 1`.

1. Clear statistics for a specific VLAN.

       SEFOS# configure terminal
       SEFOS(config)# ipv6 mld snooping clear counters vlan 1

2. Verify that snooping statistics have been cleared for `VLAN 1`.

       SEFOS# show ipv6 mld snooping statistics vlan 1

         Snooping Statistics for VLAN 1
         General queries received: 0
         Group specific queries received: 0
         Group and source specific queries received: 0
         ASM reports received: 0
         SSM reports received: 0
         IS_INCLUDE messages received: 0
         IS_EXCLUDE messages received: 0
         TO_INCLUDE messages received: 0
         TO_EXCLUDE messages received: 0
         ALLOW messages received: 0
         Block messages received: 0
         Leave messages received: 0
         General queries transmitted: 0
         Group specific queries transmitted: 0
         ASM reports transmitted: 0
         SSM reports transmitted: 0
         Leaves transmitted: 0
         Packets dropped: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |