Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable the `split-horizon` Option With Poison Reverse

1. Enter the configuration mode for the interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1

2. Enable the `split-horizon` option with poison reverse.

       SEFOS(config-if)# ip split-horizon poisson
       SEFOS(config-if)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |