Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Reset the Default Metric

1. Reset the default metric for the redistributed routes.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# no default-metric

2. Enable static route redistribution.

       SEFOS(config-router)# redistribute static
       SEFOS(config-router)# end

3. On switch 1, review the metric for redistributed RIP route entries.

       SEFOS# show ip rip database

       10.0.0.0/8 [1] auto-summary
       10.0.0.0/16 [1] directly connected, vlan1
       50.0.0.0/8 [3] auto-summary
       50.0.0.0/8 [3] redistributed via 0.0.0.0
       60.0.0.0/8 [3] auto-summary
       60.0.0.0/8 [3] redistributed via 0.0.0.0
       70.0.0.0/8 [3] auto-summary
       70.0.0.0/8 [3] redistributed via 0.0.0.0
       80.0.0.0/8 [3] auto-summary
       80.0.0.0/8 [3] redistributed via 0.0.0.0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |