Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable IPv6 Routing

1. Enter Global Configuration mode.

       SEFOS# configure terminal

2. Enable IPv6 unicast routing in the interface.

       SEFOS(config)# ipv6 unicast-routing
       SEFOS(config)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |