Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

#### Enabling a Particular VLAN Name

The VLAN name TLV transmission status is disabled by default. If you configure a new VLAN with a VLAN or the existing VLAN name is changed, the TLV transmission status of the VLAN name is disabled by default. Use one of the procedures in this section to enable a new VLAN name or to re-enable an existing VLAN name.

These procedures show how to enable a particular VLAN name:

- Enable a New VLAN Name

- Enable an Existing VLAN Name

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |