Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Settings

The following table shows the default settings for IGMP configuration parameters.

Feature | Default Setting
--- | ---
IGMP status | Disabled
IGMP fast leave | Disabled
IGMP version | 2
IGMP query interval | 125 seconds
IGMP max response time | 100 seconds
IGMP robustness value | 2
IGMP last member query interval | 10 seconds
Debug level | None
IGMP proxy | Disabled
IGMP proxy mrouter timeout | 125 seconds
IGMP proxy mrouter version | 3

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |