Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

## Add a Tagged VLAN

- Add `vlan 3` as tagged to port `0/3`.

      SEFOS# configure terminal
      SEFOS(config)# vlan 3
      SEFOS(config-vlan)# ports add extreme-ethernet 0/3
      SEFOS(config-vlan)# exit

##### Related Information

- Add an Untagged VLAN

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |