Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Add a RIP Neighbor

In this example, switch 2 is added to switch 1.

1. On switch 1, enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1

2. Add the switch 2 as a neighbor.

       SEFOS(config-router)# neighbor 10.0.0.2
       SEFOS(config-router)# end

   In switch 1, you should be able to view only the routes that are sent as RIP updates from the neighbor router (switch 2 at `10.0.0.2`).

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |