Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

## Create SLB-L2 Server Members

When you add a member as the first member of a group, an SLB-L2 group is created. The following example shows adding active port members to an SLB-L2 group.

1. Add the first active port member to the group.

       SEFOS# configure terminal
       SEFOS(config)# slb l2 1 extreme-ethernet 0/3-5
       SEFOS(config)# end

2. Show current SLB-L2 groups and members.

   The following example shows one SLB-L2 group with three active SLB-L2 port members and one standby SLB-L2 port member.

       SEFOS# show slb l2

       L2 SLB Group #1:
               Failover Method: Failover to All Ports
       Port Members:
       Port    State     Comments
       ====    =====     ==================
       3       ACTIVE
       4       ACTIVE
       5       ACTIVE
       6       STANDBY

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |