Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Install the Battery

1. Remove the battery.

   See Remove the Battery.

2. Unwrap the replacement battery from its antistatic packaging.
3. Install the replacement battery into the main board with the + side up.
4. Orient the cover over the switch and lower it in place.
5. Slide the cover forward so that it engages at the front panel.

   Ensure that the screw holes in the cover align with the holes in the switch.

6. Use a No. 1 Phillips screwdriver to install the 16 screws that secure the cover to the switch.
7. Use eight screws to attach the two post brackets to the rear sides of the switch chassis.
8. Use eight screws to attach the two rail brackets to the front sides of the switch chassis.
9. Install the switch into the rack.

   See Installing the Switch.

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |