Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Configurations

Feature | Default Setting
--- | ---
DHCP server status | Disabled
ICMP echo | Disabled
Offer reuse time out | 5 seconds
DHCP next server address | 0.0.0.0 (none)
Boot file name | Blank (none)
DHCP server pool lease time | 3600 seconds
DHCP server pool utilization threshold | 75%
DHCP server debug level | None
DHCP relay status | Disabled
DHCP relay server address | 0.0.0.0 (none)
RAI option | Disabled
DHCP relay debug level | 0x1

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |