Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Reset the Version

1. Enter the configuration mode for the interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1

2. Reset the version.

       SEFOS(config-if)# no ip rip send version
       SEFOS(config-if)# no ip rip receive version

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |