Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VRRP Administration Guide

Search Scope:

- This Document
- Entire Library

### CLI Command Modes

The following table lists the configuration modes used in this document with their access and exit methods.

Command Mode | Access Method | Prompt | Exit Method
--- | --- | --- | ---
User EXEC | Access SEFOS from Oracle ILOM with read-only rights (privilege level 1). | `SEFOS>` | Use logout or exit to return to the Oracle ILOM prompt.
Privileged EXEC | Access SEFOS from Oracle ILOM with full administrative rights (privilege level 15). | `SEFOS#` | Use the `logout` or `exit` command to return to the Oracle ILOM prompt.
Global Configuration | From User EXEC mode, use the `enable` command. | `SEFOS(config)#` | Use the `end` command to return to Privileged EXEC mode.
Interface Configuration | From Global Configuration mode, use the `interface` `interface-type interface-id` command. | `SEFOS(config-if)#` | Use the `exit` command to return to Global Configuration mode, or use the `end` command to return to Privileged EXEC mode.
VRRP Router Configuration | From Global Configuration mode, use the `router VRRP` command. | `SEFOS(config-vlan)#` | Use the `exit` command to return to Global Configuration mode, or use the `end` command to return to Privileged EXEC mode.
VRRP Interface Configuration | From VRRP Router Configuration mode, use the command `interface vlan vlan-id` command. | `SEFOS(config-vrrp-if)#` | Use the `exit` command to return to Global Configuration mode, or use the `end` command to return to Privileged EXEC mode.

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |