Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Create Forbidden Ports

The `forbidden` setting prevents the port from participating in the specified VLAN activity. This setting also ensures that any dynamic requests for the port to join the VLAN are ignored. In the following example, ports 0/2-5 are added to VLAN 2, and port 0/1 is assigned the `forbidden` tag.

1. Enter the configuration mode for the VLAN.

       SEFOS# configure terminal
       SEFOS(config)# vlan 2

2. Create a forbidden port.

       SEFOS(config-vlan)# ports extreme-ethernet 0/2-5 forbidden extreme-ethernet 0/1
       SEFOS(config)# end

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |