Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Log Into Oracle ILOM CLI (NET MGT)

1. Obtain the IP address or host name of your SP.

   See:

   - Verify the DHCP-Assigned IP Address and Host Name

   - Configure Network Management From CLI (SER MGT)

2. Configure an externally accessible IP address on the switch.

   Perform the appropriate task described in Connecting to the Service Processor.

3. Start your SSH client.
4. Log in to the switch Oracle ILOM.

       $ ssh ipaddress -l root

   where ipaddress is the IP address of the switch.

5. Type your password when prompted.

   The default is `changeme`.

   The CLI command prompt appears.

       ->

6. Access SEFOS.

   See Connect to SEFOS.

##### Related Information

- Oracle ILOM Overview

- Verify the DHCP-Assigned IP Address and Host Name

- Configure Network Management From CLI (SER MGT)

- Log Into Oracle ILOM Web (NET MGT)

- Log Into Oracle ILOM CLI (SER MGT)

- Configure Network Management From Web

- Configure Network Management From CLI (NET MGT)

- Log Out of ILOM

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |