Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring GVRP

GVRP is an application defined in the IEEE 802.1Q standard that is used to control VLANs. With GVRP, a single switch is manually configured with all the desired VLANs for the network, and all other switches on the network learn those VLANs dynamically. GVRP is enabled by default in Oracle’s SEFOS.

This section contains two examples of how to configure GVRP. In both examples, two switches are connected back-to-back using one port on each switch.

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |