Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default LAN Delay Interval

This example restores the default LAN message propagation interval to 0.

- Restore the default LAN delay value.

      SEFOS# configure terminal
      SEFOS(config)# no ip pim lan-delay
      SEFOS(config)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |