Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable Static RP

Static RP is disabled in the system, by default. Complete the following task to enable static RP.

1. Enable a static RP.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim enable
       SEFOS(config)# set ip pim static-rp enable
       SEFOS# end

2. Ensure that the static RP has been enabled.

       SEFOS# show ip pim rp-static

       Static-RP Enabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |