Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Examine the Configuration Details in SEFOS9

- Type.

      SEFOS# show ip ospf database nssa-external

      OSPF Router with ID (10.2.2.9)
                        NSSA External Link States (Area 0.0.0.2)
                        ----------------------------------------------
      LS age             : 300
      Options            : (No ToS Capability, DC)
      LS Type            : NSSA External Link
      Link State ID      : 90.0.0.0
      Advertising Router : 10.2.2.9
      LS Seq Number      : 0x80000001
      Checksum           : 0xc84f
      Length             : 36

                        NSSA External Link States (Area 0.0.0.2)
                        ----------------------------------------------
      LS age             : 300
      Options            : (No ToS Capability, DC)
      LS Type            : NSSA External Link
      Link State ID      : 0.0.0.0
      Advertising Router : 10.4.0.2
      LS Seq Number      : 0x80000002
      Checksum           : 0x120
      Length             : 36
      SEFOS# show ip ospf summary-address

      Display of Summary addresses for Type5 and Type7 from redistributed routes

      OSPF External Summary Address Configuration Information
      -------------------------------------------------------
      Network        Mask           Area           Effect  TranslationState
      -------      ----            ----           ------   ----------------
      255.0.0.0     0.0.0.2        advertiseMatching     enabled

      SEFOS# show ip route

      O 0.0.0.0/0  [2] via 10.2.2.2
      C 10.2.2.0/24 is directly connected, vlan2
      O 10.4.0.0/16 [2] via 10.2.2.2
      C 12.0.0.0/8  is directly connected, vlan1
      S 90.1.0.0/16 [1] via 10.2.2.2
      S 90.2.0.0/16 [1] via 10.2.2.2
      S 90.3.0.0/16 [1] via 10.2.2.2
      S 90.4.0.0/16 [1] via 10.2.2.2
      S 90.5.0.0/16 [1] via 10.2.2.2

      SEFOS# show ip ospf route

      OSPF Process Routing Table
      Dest/Mask                  TOS NextHop/Interface Cost Rt.Type   Area
      ---------                  --- -------/--------- ---- -------   ----
      0.0.0.0/0.0.0.0            0   10.2.2.2/vlan2    2    Type1Ext  0.0.0.2
      10.2.2.0/255.255.255.0     0   0.0.0.0/vlan2     1    IntraArea 0.0.0.2
      10.4.0.0/255.255.0.0       0   10.2.2.2/vlan2    2    InterArea 0.0.0.2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |