Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### QoS Administration Guide

Search Scope:

- This Document
- Entire Library

## Set up the Ingress Policy

You can use the `policy-map` command to set up the ingress policy.

1. Linking the traffic class to a defined meter.

       SEFOS(config)# policy-map 5000
       SEFOS(config-ply-map)# set policy class 3000 default-priority-type none
       SEFOS(config-ply-map)# set meter 4001 conform-action set-ip-dscp-transmit 10 exceed-action  set-ip-dscp-transmit 12 violate-action set-ip-dscp-transmit 14
       SEFOS(config-ply-map)# exit
       SEFOS(config)# policy-map 5001
       SEFOS(config-ply-map)# set policy class 3001 default-priority-type none
       SEFOS(config-ply-map)# set meter 4002 conform-action set-ip-dscp-transmit 10 exceed-action  set-ip-dscp-transmit 12 violate-action set-ip-dscp-transmit 14
       SEFOS(config-ply-map)# exit
       SEFOS(config)# policy-map 5002
       SEFOS(config-ply-map)# set policy class 3002 default-priority-type none
       SEFOS(config-ply-map)# set meter 4002 conform-action set-ip-dscp-transmit 10 exceed-action  set-ip-dscp-transmit 12 violate-action set-ip-dscp-transmit 14
       SEFOS(config-ply-map)# exit
       SEFOS(config)# policy-map 5003
       SEFOS(config-ply-map)# set policy class 3003 default-priority-type none
       SEFOS(config-ply-map)# set meter 4000 conform-action set-ip-dscp-transmit 10 exceed-action  set-ip-dscp-transmit 12 violate-action set-ip-dscp-transmit 14
       SEFOS(config-ply-map)# exit
       SEFOS(config)# policy-map 5004
       SEFOS(config-ply-map)# set policy class 3004 default-priority-type none
       SEFOS(config-ply-map)# set meter 4000 conform-action set-ip-dscp-transmit 10 exceed-action  set-ip-dscp-transmit 12 violate-action set-ip-dscp-transmit 14
       SEFOS(config-ply-map)# exit
       SEFOS(config)# exit

2. Review the policy map information.

       SEFOS# show policy-map
       QoS Policy Map Entries
       ----------------------
       PolicyMapId      : 1
       IfIndex          : 0
       Class            : 1
       DefaultPHB       : None.
       MeterId          : 0
       ConNClass        : 0
       ExcNClass        : 0
       VioNClass        : 0
       ConfAct          : None.
       ExcAct           : None.
       VioAct           : None.

       PolicyMapId      : 5000
       IfIndex          : 0
       Class            : 3000
       DefaultPHB       : None.
       MeterId          : 4001
       ConNClass        : 0
       ExcNClass        : 0
       VioNClass        : 0
       ConfAct          : IP Dscp 10
       ExcAct           : IP Dscp 12
       VioAct           : IP Dscp 14

       PolicyMapId      : 5001
       IfIndex          : 0
       PolicyMapId      : 5003
       Class            : 3001
       IfIndex          : 0
       Class            : 3003
       DefaultPHB       : None. MeterId          : 4000
       MeterId          : 4002 ExcNClass        : 0
       DefaultPHB       : None. ConNClass        : 0
       ConNClass        : 0 ExcNClass        : 0 VioNClass        : 0 ConfAct          : IP Dscp 10 VioNClass        : 0 ExcAct           : IP Dscp 12
       ConfAct          : IP Dscp 10
       VioAct           : IP Dscp 14
       ExcAct           : IP Dscp 12
       VioAct           : IP Dscp 14
       PolicyMapId      : 5002 IfIndex          : 0
       PolicyMapId      : 5004
       Class            : 3002 IfIndex          : 0
       Class            : 3004
       DefaultPHB       : None. MeterId          : 4000
       MeterId          : 4002 ExcNClass        : 0
       DefaultPHB       : None. ConNClass        : 0
       ConNClass        : 0 ExcNClass        : 0 VioNClass        : 0 ConfAct          : IP Dscp 10 VioNClass        : 0 ExcAct           : IP Dscp 12
       ConfAct          : IP Dscp 10
       VioAct           : IP Dscp 14
       ExcAct           : IP Dscp 12
       VioAct           : IP Dscp 14
       PolicyMapId      : 5003 IfIndex          : 0
       Class            : 3003
       DefaultPHB       : None.
       MeterId          : 4000
       ConNClass        : 0
       ExcNClass        : 0
       VioNClass        : 0
       ConfAct          : IP Dscp 10
       ExcAct           : IP Dscp 12
       VioAct           : IP Dscp 14
       PolicyMapId      : 5004
       IfIndex          : 0
       Class            : 3004
       DefaultPHB       : None.
       MeterId          : 4000
       ConNClass        : 0
       ExcNClass        : 0
       VioNClass        : 0
       ConfAct          : IP Dscp 10
       ExcAct           : IP Dscp 12
       VioAct           : IP Dscp 14

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |