Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure DHCP Global Options

You can configure DHCP global options as described in this section. Global options are available to DHCP clients only when there is no host-specific option and there is no pool-specific option. The value applies to the complete DHCP pool in the specified switch.

In this example, `option 3` is the default router option for switch 1.

1. Configure the DHCP global option for the default router.

       SEFOS# configure terminal
       SEFOS(config)# ip dhcp option 3 ip 12.0.0.2
       SEFOS(config)# end

2. View the global options configured in switch 1.

       SEFOS# show ip dhcp server pools

       Global Options
       --------------
       Code       :     3, Value      : 12.0.0.2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |