Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Static Neighbor Cache Entries

The neighbor cache contains a set of entries about individual neighbors to which traffic has been sent. Each neighbor cache entry contains the information about the interface, IPv6 address, link-layer address, and reach state of the neighbors. Routers and hosts record the neighbor information in the local neighbor cache in NDP. You can add entries statically in the neighbor cache.

These procedures show how to configure static neighbor cache entries:

- Add a Neighbor Cache Entry

- Delete a Neighbor Cache Entry

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |