Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable IPv6 Routing

1. Enter Global Configuration mode.

       SEFOS# configure terminal

2. Disable IPv6 unicast routing in the interface.

       SEFOS(config)# no ipv6 unicast-routing
       SEFOS(config)# exit

3. Review the configuration information.

       SEFOS# show running-config

       interface vlan1
        ip address  12.0.0.1 255.0.0.0
        no shutdown
       !
       no ipv6 unicast-routing

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |