Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable RIPng

1. On the switch, enable IPv6 unicast routing.

       SEFOS 2 SEFOS# configure terminal
       SEFOS 2 SEFOS(config)# ipv6 unicast-routing

2. Enable RIPng and route redsitribution.

       SEFOS 2 SEFOS(config)# ipv6 router rip
       SEFOS 2 SEFOS(config-router)# redistribute connected
       SEFOS 2 SEFOS(config-router)# end
       SEFOS 2 SEFOS#

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |