Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Settings

SEFOS is shipped with the following default settings:

Feature | Default Setting
--- | ---
Port channel | Disabled
Channel groups | None
LACP system priority | 0x8000 or 32768
Load balancing | Source and destination (MAC address based)
LACP wait time | 2
LACP timeout | Long (The LACP PDU is sent every 30 seconds, and the LACP timeout value is sent every 90 seconds.)
MAC selection | Dynamic (The port-channel MAC address is the address of an active port.)

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |