Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default External Database Limit

This example restores the default external database limit to -1 (no limit) for SEFOS1 (router `10.0.0.1`).

Note - The exit overflow interval will be 0 until you configure it.

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in the switch SEFOS1.

       SEFOS(config)# ipv6 router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.0.0.1

4. Configure the external LSDB limit.

       SEFOS(config-router)# as-external lsdb-limit -1

5. Exit Router Configuration mode.

       SEFOS(config-router)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |