Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default Delay Time

This example restores the default delay time (5 seconds) and hold time (10 seconds).

- Restore the default delay and hold times.

      SEFOS(config-router)# no spf timer

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |