Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Install a Fan

1. Remove a fan.

   See Remove a Fan.

2. Verify that the slot where the fan installs is clean and free of debris.
3. Orient the fan over the opening in the switch chassis with the thumbscrew on the right.
4. Firmly slide the fan into the switch until the fan stops.

   The fan might immediately power on.

5. Tighten the captive thumbscrew to secure the fan in the switch chassis.
6. Verify that the fan Attention LED is no longer illuminated.
7. Verify the fan operation.

##### Related Information

- Remove a Fan

- Install a Power Supply

- Install an Ethernet Cable

- Install the Battery

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |